FREE DELIVERY!

The Boom Arm 5Mt will let hose and cord out of the way eliminating tripping hazard and protecting your workpiece from damage. Boom arm eliminates snags, helping you tackle large workpieces with ease and efficiency. Simplifies the work process so you can focus on your workpiece,not on hose and cord management .On the market you can find it for about £3500! Nothing can compete for price and quality .This is not a chinese product! Connect any automatic dust extractor or hoover and your workstation it is ready!

Items Included

double-jointed arm with wall bracket

cable duct

in carton;

The Boom arm 5mt assembled with Energy Box 220V, 2 sockets, 2 pneumatic inlets, 2

Tools Holders, 2 Suction inlets, Power Plug and pneumatic Plug

The Dust Extractor is not included. Brand New Material

For large working areas.

• Saves time, space and increases economic efficiency

• Maximum flexibility, extra safety, no dangerous obstacles

• Installation on a wall or pillar possible

• Expands the range up to 84 m²

• For use with Festool CT/SRM mobile or any dust extractors

• Integrated compressed air and electrical lines for connection to EAA and CT

Main areas of use

• For use with any mobile or fixed dust extractors

• Ergonomic and flexible layout of workplaces

Technical data

Connecting line length 3 m

Boom extension 2 x 2.5 m

50 - 80 m² (about)

weight 45 kg (about)